APPENDIX E

COMMISSIONING TEST REPORT

(Informative)

**THE FIRE DETECTION AND ALARM SYSTEM   
 INSTALLED AT:**

(Premises) …………………………………………..…………………………………..…

……………………………………..……………………………………………

……………………………………………..……………………………………

Postcode ………………………………………

Owner or Owner's Authorized Agent ……………………………………..….…………………....

………………………………………… …...……...……………………………………………….

……………………………………… …...…………...…...………………………………………..

…………………………………… ……...…………………………………………………………..

……………………………………...……………………………...………………………………..

Postcode……………..…………………………...

NEW\*

MODIFICATION TO SYSTEM~~\*~~   
ADDITION TO~~\*~~

(\*Cross out those not applicable)

Date of commissioning tests ……………………….……….…………………………………

Name and address of commissioning company, company stamp or company (name in...

'BLOCK LETTERS') …………………………………………………………………………………

………………………………………………………………… ……………………..…………… ………………………………………………………………………… ……………………………. …………………………………………………………………………………………………………

……MAILING:………. ………………………………………… ………………………………….. …………………………………………………………… …….……………………………………. …………………………………………………………………………………………………………

Postcode……………..…………………………

Commissioning person

Name (print)…… ……… …………………………...........................

Signature

INSTRUCTIONS:

This form is to be used in conjunction with-

(a) operator's manual;

(b) installer's statement(s); and

(c) 'as-installed' drawings,

to provide a complete description of the installed system and its tested performance at the

time of its commissioning into service.

**SYSTEM INFORMATION**

**GENERAL YES NO N/A**

(a) Equipment has been designed and constructed in

accordance with the relevant Standards.

(b) Installation Equipment has been located, installed and interconnected

in accordance with the system documentation.

(c) Compatibility All detectors and other devices used in the system are-

(i) listed in the operator's manual:

(ii) compatible with the relevant parts of CIE, particularly that the

permitted number of detectors and other devices for each circuit

is not exceeded.

(iii) installed in an environment for which they are suitable.

(iv) not set to a sensitivity outside that prescribed in the relevant

product Standard.

(d) Alarm zone limitations The alarm zone limitations in Clause 2.4 of

AS 1670.1 are not exceeded.

(e) Primary power source

(i) The primary power source for the system has been provided in

accordance with AS/NZS 3000.

(ii) The isolating switch disconnects all active conductors.

(iii) Five operations of the primary power source switch did not

cause an alarm to be indicated on the system.

(f) Secondary power source

(i) The secondary power source is of a suitable type and capacity

complying with the requirements of Clause 3.16.2 of AS 1670.1.

(ii) The float voltage, charger type and setting is correct and in

accordance with the battery manufacturer's recommendation.   
(g) Battery temperature and voltage The battery voltage corresponds to

that specified by the battery manufacturer for the temperature

measured after 24 h quiescent operation.

(h) Alarm zone parameters Each alarm zone circuit is within the

equipment manufacturer's specifications.

**YES NO N/A**

(i) Wire-free alarm zones Wire-free actuating device parameters meet

the minimum parameters specified by the manufacturer, including that

the receiver responds to signals from an actuating device for alarm,

tamper, low standby power signals and gives a fault signal when the

supervisory signal condition is absent.

(j) Operation of fault and alarm signals Fault and alarm conditions

correctly detect and indicate as the correct alarm zone, operating

other required indicators, and operate relevant outputs of the CIE.

(k) Mimic panel All mimic panels, annunciators. etc.. operate correctly.

(I) Alarm zone controls Alarm test, fault test, isolate and reset facility of

each alarm zone operates correctly.

(m) Alarm dependency Alarm dependency works correctly and does not

apply to devices listed in Clause 3.3 of AS 1670.1.

(n) CIE response to actuating device operation. Each actuating device

has operated when tested with a medium suitable for the device type

and the alarm has indicated on the FIP and at the tested device.

(o) Fault response time. The response to a fault does not exceed 100 s

for each alarm zone circuit.

(p) Alarm response time At least one detector in each alarm zone has

been tested and the response to the alarm does not exceed 10 s or

the period specified when dependency on more than one alarm signal

is used.

(q) Supervisory signal response time At least one supervisory device in

each alarm zone circuit has been tested and the response to the

supervisory device does not exceed 100 s.

(r) Alarm acknowledgment facility Alarm acknowledgement facilities

operate in accordance with the requirements of Clause 3.2 AS 1670.1

(s) Occupant warning system

(i) A fault signal is displayed at the CIE when the circuit wiring at

the last speaker or sounder is short or open circuited.

(ii) Each sounder/speaker operates in accordance with the

requirements of Clause 3.22 of AS 1670.1 and a record of the

sound pressure level has been made.

(t) The external alarm indication is visible from the main approach to the

building.

(u) Manual call points

(i) Each manual call point operates correctly.

(ii) The activation of manual call points do not cause existing

detector alarm indications to be extinguished.

**YES NO N/A**

(iii) Manual call points are not subject to alarm dependency.

(v) Smoke and fire door release Each door-release device operates

correctly.

(w) Flame detectors

(i) The number and type of flame detectors provide adequate

protection for the area.

(ii) There are no 'blind' spots in the area protected.

(iii) Detectors are rigidly fixed.

(iv) Detector lenses are clean and adequately protected from dust    and extraneous radiation sources.

(v) Detectors respond to a flame or simulated flame source.

(x) Multi-point aspirating smoke detectors

(i) Response time of all sampling points meets the requirements of

AS 1670.1.

(ii) Alarm settings and indicators operate correctly.

(iii) Remote indication of alarm and fault signals operate correctly.

(iv) Airflow failure indicator operates correctly.

(v) System (signal) failure indicators operate correctly.

(vi) Isolate and reset functions operate correctly.

(vii) Alarm and fault test facilities operate correctly.

(y) Duct sampling unit The alarm indicator is clearly visible from a

trafficable area and the duct air velocity exceeds the minimum velocity

specified for the unit. If not, the measured differential pressure is at

least the minimum specified for the unit

(z) Ancillary control functions Each ancillary control function operates

with the activation of associated alarm zones.

(aa) Alarm signaling equipment Alarm signaling equipment initiates a fire

alarm signal to the monitoring service provider.

(bb) Labeling Alarm zone location is immediately apparent from the alarm

zone labeling.

**DOCUMENTATION**

The following documentation is located in or adjacent to the FIP:

**YES NO N/A**

(a) 'As-installed' drawings

(b) CIE documentation required by AS 4428.1 or AS 7240.2.

(c) Commissioning test report.

(d) Installer's statement in accordance with Appendix E of AS 1670.1.

(e) A log complying with the requirements of Clause 7.3 of AS 1670.1.

(f) Aspirating system design tool calculation.