

**FIRE ALARM MONITORING SERVICES**

**TEST MODE**

**To disable communication to DFES Communication Centre**

**Step 1:** Place the iButton onto the reader for 3-4 **Step 2:** Display will show Testmode seconds. 240m





**The ASE will automatically exit Test Mode 4 hours after entering Test mode, unless manually returned to normal mode ‘AS1670.3-2018’**

F1 – Not in Use

Comms Path 2 – Not in Use

**RETURNING THE ASE BACK TO NORMAL MODE**

**To enable communication with DFES Communication Centre**

1. Reset all Alarms on the Fire Indicator Panel (FIP).
2. Press the F2 button for 1-2 seconds on the ASE to clear “ALARM STATUS” Alarms that are in the ASE memory.
3. Place the iButton on the reader for 3-4 seconds to change the ASE from the Test Mode to the Normal Mode "AS1670.3-2018".

**Removing the ASE from the Test Mode with active Alarms will call the Fire Brigade!**

FOR ASSISTANCE PLEASE CONTACT   
FIRE ALARM MONITORING SERVICES 24/7 ON:

**1300 793 722**